## Setting the IP address

Follow the procedure below to set the device IP address:

1. Click Device Setting Button()to open the setting window.
2. Select the appropriate IP acquisition method from the choices displayed.
3. If you choose Manual, you can manually configure the settings.
4. Enter appropriate values in the fields for the IP Address, Subnet Mask and Default Gateway Address.
5. Click [OK].
6. If the Enter Password window is shown, enter the appropriate password to confirm the settings.
7. The device supporting Configuration Tool will be add to the Configuration Tool database automatically after configuration.
8. The information of device that already added to the Configuration Tool database will be updated automatically after configuration.
9. The device not supporting Configuration Tool will not be added to the Configuration Tool database after configuration.
10. If you need to restart the device following the setup, click [OK] on the Setup Complete windows.
11. If you do not want to restart the device immediately, click [Cancel] to close the window. Use the Restart function when you need to restart the device later.